**H.B.T.I Kanpur**

**Tender Form**

Name of work- **Renovation of GH-I hostel east campus**

Estimated cost- Rs 1925731.00

Time of completion-03months Earnest money- Rs 40000.00 Tender form cost- Rs 2300.00

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl.No.** | **Schedule Item** | **Description Of Work** | **Quantity** | **Rate Rs** | **Amount Rs** |
| 1 | 706 | Dismantling of existing plaster including disposal of refuse material within a distance of 60M | 200 Sqm |  |  |
| 2 | 17.91 | 15 mm thick plaster 1:3 cement and coarse sand plaster in ceiling | 150 Sqm |  |  |
| 3 | 17.59(iii) | 15 mm thick plaster 1:6 cement and coarse sand plaster on walls | 50 Sqm |  |  |
| 4 | 301 | P/F of first quality Indian type white glazed ISI marked WC pan with cistern etc. complete | 03 Nos |  |  |
| 5 | 502(B) | MS or iron work in steel Z section repairing/replacing windows, doors etc including supply of all materials | 250 Kg |  |  |
| 6 | 812(B) | Fixing panes of glass with equal or equivalent ISI mark quality with putty brads and springs and including supply of material and labour etc complete work 3.8 to 4.7 mm thick | 60 Sqm |  |  |
| 7 | MR | Approximate cost of ISI marked oxidized iron fitting with screws for door and windows etc. | 50 Set |  |  |
| 8 | 305 | M-150B/W in 1:4 cement and coarse sand in SS including necessary cutting and molding of brick as required for walls | 12.5 Cum |  |  |
| 9 | 671 | White washing one coat including supply of all materials, labour T&P etc. required for proper completion of work | 200 Sqm |  |  |
| 10 | 675 | colour washing two coat including supply of all materials, labour T&P etc. required for proper completion of work | 12702 Sqm |  |  |
| 11 | 643 | Painting/Varnishing old work in small areas of old wood work with one coat of ready mixed priming paint and two coat of approved superior quality ready mixed paint or varnish including supply of all materials labour T&P etc. required for proper completion of work. Paint to be used should confirm then ISI No. 103,1950 | 3010 Sqm |  |  |
| 12 | 662 | Applying acrylic emulsion two coats of Asian or equivalent make for outer surface | 3979 Sqm |  |  |
| 13 | 470(A) | S/F 32mm thick flush door single leaf commercial quality conforming of IS2202 part I (1983) including fixing of wooden cleats and stoppers and including fixing and adjustment of hinges bolts locks handles springs fitting with necessary screws to be supplied departmentally | 96 Sqm |  |  |
| 14 | 641 | Painting/Varnishing new work in small areas of new wood work with one coat of ready mixed priming paint and two coat of approved superior quality ready mixed paint or varnish including supply of all materials labour T&P etc. required for proper completion or work. Paint to be used should confirm the ISI No. 103,1950. | 188 Sqm |  |  |
| 15 | 708 | Scraping old white or colour washes including disposal of refuse material within a distance of 60m | 7690 Sqm |  |  |
| 16 | MR | S/F red granite slab not less than 2Cm thick on service platform etc. with rounding the edges etc. complete | 15 Sqm |  |  |
| 17 | 644 | Distempering two coats with O.B.D of approved brand and manufacturer and of required shade on previously painted surface such as Berger, Asian paints J&N Shalimar after thoroughly brushing the surface free from dust and other foreign matters including its sand papering and cleaning the surface | 437.82 Sqm |  |  |
| 18 | MR | P/L JK/Birla white wall putty | 995 Sqm |  |  |
| 19 | MR | S/F MS chowkhat | 180 Kg |  |  |
| 20 |  | Electrification work 12.5% |  |  |  |
| 21 |  | Plumbing work 10% |  |  |  |
| 22 |  | Contingency 5% |  |  |  |
|  |  |  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Renovation of GH-I hostel east campus**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**