**H.B.T.I Kanpur**

**Tender Form**

Name of work- **Renovation work in GH-III hostel east campus**

Estimated cost- Rs 1431900.00

Time of completion- 02 months Easrnest money- Rs 30000.00

Tender form cost- Rs 1700.00

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl.No.** | **Schedule Item** | **Description Of Work** | **Quantity** | **Rate Rs** | **Amount Rs** |
| 1 | 706 | Dismantling of existing plaster including disposal of refuse material within a distance of 60M | 25 Sqm |  |  |
| 2 | 17.91 | 15 mm thick plaster 1:3 cement and coarse sand plaster in ceiling | 65 Sqm |  |  |
| 3 | 17.59(iii) | 15 mm thick plaster 1:6 cement and coarse sand plaster on walls | 25 Sqm |  |  |
| 4 | MR | Approximate cost of ISI marked oxidized iron fitting with screws for door and windows etc. | 22 Set |  |  |
| 5 | 708 | Scraping old white or colour washes including disposal of refuse within a distance of 60m(60% whole of painting area) | 4137.5Sqm |  |  |
| 6 | 660 | Finishing wall with water proofing cement paint of approved and quality on new work with two coat to give an even shade, including supply of all material labour and T&P etc. required for proper completion of the work | 1988 Sqm |  |  |
| 7 | 649 | One priming coat and one coat oil distemper on new work including supply of all material labour and T&P etc. required for proper completion of the work | 4906 Sqm |  |  |
| 8 | 650 | As in item 649 above but for every coat after the first coat | 4906 Sqm |  |  |
| 9 | Chap 24 | Supply of material for MS steel or iron window including necessary fittings for hinges, handles and sliding bolts & fastner   1. MS angle 25x25x5 mm 2. MS flat 5mm thick | 4725 Kg |  |  |
| 10 | Chap 1/16 | Supply of SS mosquito proof jali | 280 Sqm |  |  |
| 11 | 502 | Labour rate for fabrication of MS mosquito window complete | 4725 Kg |  |  |
| 12 | MR | Fixing of mosquito frame up to 2.50m with hole fastener | 125 Nos |  |  |
| 13 | Chap 24 | MS work for open back yard area at bathroom for safety purpose   1. MS angle 25x25x5 mm 2. MS bar 5mm | 220 Kg |  |  |
| 14 | 502 | Fabrication | 220 Kg |  |  |
| 15 | MR | Fixing of MS grill with mason work | 220 Kg |  |  |
| 16 | Chap 1+25 | S/F of PVC drain pipe 110mm dia. ISI marked with proper MS clamping including all mason work for making proper water drainage as per departmental requirement | 581 Rm |  |  |
| 17 | Chap 1 | S/F of PVC bend 100mm for Sl. no. 16 work | 187Nos |  |  |
| 17 | MR | P/L one coat wall putty(J.K/Birla) in proper way | 310 Sqm |  |  |
| 18 | 812 | Fixing panes of glasses with equal or equivalent ISI marked putty. Brads and springs and including supply of all material (2.8 to 3.7mm thick) | 110 Sqm |  |  |
| 19 | Chap 21 | S/F of GI pipe   1. 15mm dia. 2. 25mm dia. | 35 Rm  20 Rm |  |  |
| 20 | Chap 21 | GI Fitting and water tapes | LS |  |  |
| 21 | Chap 21,22,23 | S/F of complete hand wash basin | 04 No |  |  |
| 22 | Chap 22 | Looking mirror of Atul make with Indian polish of 600×450mm dia size with beveled edge | 06 No |  |  |
| 23 | 470(A) | S/F 32mm thick flush door single leaf commercial quality conforming of IS2202 part I (1983) including fixing of wooden cleats and stoppers and including fixing and adjustment of hinges bolts locks handles springs fitting with necessary screws to be supplied departmentally | 40 Sqm |  |  |
| 24 | 641 | Painting/Varnishing new work in small areas of new wood work with one coat of ready mixed priming paint and one coat of approved superior quality ready mixed paint or varnish including supply of all materials labour T&P etc. required for proper completion or work. Paint to be used should confirm the ISI No. 103,1950. | 336 Sqm |  |  |
|  |  | **Total (Sl no.1 to 27)** |  |  |  |
|  |  | Electrification work 12.5% |  |  |  |
|  |  | Unseen & contingency 5% |  |  |  |
|  |  | **Grand Total** |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Renovation work in GH-III hostel east campus**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**