**H.B.T.I Kanpur**

**Tender form**

Name of work **- Renovation Work In WCH-III Hostel At West Campus**

Estimated cost- Rs 2283360.00

Time of completion- 03 months Earnest money- Rs 46000.00

Tender form cost- Rs 3000.00

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl.No.** | **Schedule**  **No.** | **Description of work** | **Quantity** | **Rate**  **(In Rs)** | **Amount**  **(In Rs)** |
| 1 | 692 | Dismantling of brick work | 14Cu.M |  |  |
| 2 | 307,310 | Class work 150 brick work in 1: 3 cement and coarse sand mortar | 07Cu.M |  |  |
| 3 | 706 | Dismantling of existing plaster | 400Sqm |  |  |
| 4 | 17.59(II) | 15mm thick plaster 1 cement : 4 fine sand | 400Sqm |  |  |
| 5 | 251 | Earth work in excavation | 12Cu.M |  |  |
| 6 | 275 | P/L in cement concrete 1 : 4 : 8 (1cement : 4 fine sand : 8 graded brick aggregate 40mm) | 02Cu.M |  |  |
| 7 | MR | S/F plastic door complete make sintex, century or eqv. | 115Sqm |  |  |
| 8 | MR | S/F plastic chaukhat complete make sintex, century or eqv. | 380RM |  |  |
| 9 | 628 | S/F 5mm thick china glazed tile in wall with 1:3 cement and coarse sand mortar with complete work | 225Sqm |  |  |
| 10 | 651 | Oil bond tow coat | 200Sqm |  |  |
| 11 | MR | P/L one coat wall putty (JK/Birla) in proper way | 200Sqm |  |  |
| 12 | 289 | RCC work in columns in  1 : 1.5 : 3 with 3/4" approved stone | 01Cu.m |  |  |
| 13 | 504 | Mild steel in RCC work | 118Kg |  |  |
| 14 | MR | Teen shade with profile sheet (0.45mm) ISI mark make Tata or eqv with require structure, trusses, pillars and necessary support complete work including primar and painting | 330Sqm |  |  |
| 15 | As per analysis | P/L 80mm thick CC pre rubber molded inter locking paver tiles including 40mm thick fine sand bed over compacted base of GSB and CC work inside of interlocking tiles for proper slop and camber including all labour, T&P etc. required for proper completion of work | 455Sqm |  |  |
| 16 | 14.24 | P/L checkered terrazo tile 20mm | 06Sqm |  |  |
| 17 | 14.43(b) | P/L 20mm thick Kota stone flooring over 20mm thick base of cement mortar 1 : 4 (1cement : 4 coarse sand) laid over jointed with grey cement slurry mixed with pigment to match the shade of slab rubbing and polishing complete | 50Sqm |  |  |
| 18 | MR | S/F of Granit with polishing | 2.5Sqm |  |  |
| 19 | 502(II)+MR | S/F of MS frame with S.S. net made by MS flat (12mm width 5mm thick) in window with painting. Frame size (1.1×0.52 Sqm) approx weight 1.6Kg | 55Nos. |  |  |
| 20 | MR | S/F of S.S. net in door with dismantling of old net | 10Sqm |  |  |
| 21 | 643 | Painting two coat | 120Sqm |  |  |
| 22 | MR | S/F of RCC main hole cover with MS collar dia 400mm | 12Nos |  |  |
| 23 | 812(a) | S/F of panes of glass (2.8 to 3.7)mm thick | 200Sqm |  |  |
| 24 | MR | S/F of exhaust fan (9") with frame, make Havells/Basnsal or eqv | 08Nos |  |  |
| 25 | MR | S/F of Door closer | 02Nos |  |  |
| 26 | Chap. 21,22,24 | S/F of sink (24"×18"×10") with waste jali, drain pipe, CP cock, MS bracket complete work | 02Nos |  |  |
| 27 | Chap. 21,22,24 | S/F of wash basin (550×400)mm with drain pipe, PVC connection, waste coupling, CP pillar cock, CP stop cock, MS bracket complete work | 08Nos |  |  |
| 28 | Chap. 21,22,24 | S/F of cistern 10 Ltr. with MS bracket, CP stop cock, PVC connection complete work | 08Nos |  |  |
| 29 | Chap. 21,22,24 | S/F of urinal with drain pipe, CP stop cock, PVC connection complete work | 09Nos |  |  |
| 30 | 22,23 | S/F of looking mirror 600×450 with hard board sheet | 20Nos |  |  |
| 31 | MR | Repairing of water cooler and RO plant | 03Nos |  |  |
| 32 | MR | Supply of rickshaw trolley in wooden body (Size 50"×35"×18"×1" ), frame and parts KW make or eqsv and three wheels in solid state and GI sheet in bottom with body painting | 01Nos |  |  |
| 33 | MR | Cleaning of all 10Nos main holes, sewer lines, shook pit and drain lines | LS |  |  |
| 34 | - | Electrification work | LS |  |  |
|  |  |  |  | **Total** |  |
| 35 | - | Contingency/Unseen work 5% |  |  |  |
|  |  |  |  | **G. Total** |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non- responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Renovation Work In WCH-III Hostel At West Campus**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**