Tender Form

Name of Work-**Repair of hostel (LV- III New) at East Campus, HBTI, Kanpur.**

 Estimated Cost-Rs.1450170=00

Time of Completion – 03 months Earnest Money-Rs.30000=00

Tender Form Cost- Rs.1700=00

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sl. No.** | **Description** | **Qty.** | **Rate** | **Total Amount** |
| 1. | Dismantling lime or cement concrete work including stacking of dismantled materials with in 60 m. distance as directed by E/I. | 25 sqm |  |  |
| 2. | Cement Concrete with 2cm Gauge approved stone grit, coarse sand and cement in the proportion of 4:2:1 including supply of all materials, labour& plant etc. required for proper completion of work. | 25 cum |  |  |
| 3. | Excavation in foundation in ordinary soil (loam clay or sand)including lift up to 1.50 M and lead up to 30M. And including filling, watering and ramming of excavated earth into the trenches or into the space between the building and the sides of foundation trenches or into the plinth and removal and disposal of surplus earth as directed by the Engineer incharge upto a distance of 30M from the foundation trenches for Kota Stone. | 176.11cum |  |  |
| 4. | Cement Concrete with 4cm Gauge approved stone ballast coarse sand and cement in the proportion of 8:4:1 including supply of all materials, labour& plant etc. required for proper completion of work. For Kota Stone. | 41.238 cum |  |  |
| 5. | S/F of Kota stone in flooring 2cm (¾”)thick & joints filled with 1:2 one part cement two part of approved coarse sand with approved colouring materials to be given an even shade with12mm base coat (bedding) of 1:2 cement & coarse sand mortar & or directed by the E/I & polished by hand or machine & finally finished with French Mansion polish or any other approved polish & including supply of all materials, labour, T & P etc. required for proper completion of work excluding base concrete.  | 274.92sqm |  |  |
| 6. | Rain Water Harvesting including two manholes complete including supply of all materials, labour& plant etc required for proper completion of work. size 6x3x3. | One no. |  |  |
| 7. | Bore for handpump 4" including supply of all materials, labour& plant etc. required for proper completion of work. | One no. |  |  |
| 8. | Construction of drain 300x200mm complete with 100 mm PCC, plaster with neat cement, including supply of all materials, labour ,& plant etc.required for proper completion of work . | 60 RMtr |  |  |
| 9. | M.S. or iron work of small size & section such as holding down bolts, hold fast, tied grating etc. wrought to required form including supply of steel bolt, nuts, wastage etc. & their fixing required for proper completion of the work but in **M.S. Grills & stair case railing.** | 3000 kg |  |  |
| 10. | Renewing panes of glass in door, windows & ventilator or fixing in the new work with 4 mm thick glass panes fixed with brads & putty including supply of all material, labour and tools and plants etc. required for proper completion of work. | 50 sqm |  |  |
| 11. | Repairing of almirah door locks with locking complete including supply of all material, labour and tools and plants etc. required for proper completion of work. As per bill basis. | One job |  |  |
| 12. | Repairing of all bathrooms for seepage in adjacent rooms & flushing cisterns including supply of all material, labour and tools and plants etc. required for proper completion of work. As per bill basis. | One job |  |  |
| 13. | Providing and fixing in position collapsible steel shutter with vertical channels 20x10x20mm (⅜”x¾”) & braced with flat iron diagonals 20x5mm(¾x3/16 ) size with top & bottom rails of T iron 40x40x6mm (1½”x1½”) with 38mm dia steel pulleys with bolts, nuts, locking arrangement, stoppers, handles complete including applying a priming coat of approved lead paint. 5x3.5, 1.6x2.5 &1.6x2.5 | 25.5 sqm |  |  |
| 14 | Supply & fixing of 4Cm. Thick C.P. teak wood door & window shutters with panels of heavy quality Galvanized Mosquitos proof heavy quality iron wire gauge iron wire gauge 2.5mm or 2mm or 1.5mm mesh or any other size, with necessary beading including supply & fixing of wooden cleats & stops & including fixing & adjustment of hinges, bolts, locks, handles, spring & other fittings but excluding their supply & including painting with two coats of black Japan on all iron fitting if necessary, including fixing the glass panes with putty & brad Glass to be 4 mm thick, fitting with necessary screws to be supplied by the deptt. | 10.29 sqm |  |  |
| 15. | Providing & fixing CP Brass shower heavy quality 100mm. dia including CP brass stop cock heavy quality 15mm dia ISI marked including supply of all material, labour and tools and plants etc. required for proper completion of work and also including cutting & threading the pipe as required. | 16 no. |  |  |
| 16. | Renewing panes of glass in door, windows & ventilator or fixing in the new work with 6 mm thick glass panes fixed with Aluminum beading including supply of all material, labour and tools and plants etc. required for proper completion of work in **Aluminum Doors.** | 2.86 sqm |  |  |
| 17. | Repairing of all switch boards, fixing of flood lights- 06 nos., sodium lights-04, exhaust fan- 04 nos., tube lights etc. complete with cutting hole for exhaust fan & making good the wall including supply of all material, labour and tools and plants etc. required for proper completion of work. As per bill basis. | One job |  |  |
| 18. | Construction of approach road (hostel to Nawabganj road) 38x3 mtr. complete with earth work, l/c-6" & PCC-6" (1:2:4) including supply of all materials, labour ,& plant etc. required for proper completion of work . | One job |  |  |
| 19. | Unforeseen items. As per bill | LS |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Repair of hostel (LV - III New) at East Campus, HBTI, Kanpur.**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**