**H.B.T.I Kanpur**

**Tender Form**

Name of work- **Connection of 10 HP submersible pump 2 Nos to OHT in both campus**

Estimated cost- Rs 615906.00

Time of completion- 02 months Earnest money- Rs 13000.00

Tender form cost- Rs 1100.00

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.No.** | **PWD Sch.** | **Description** | **Qty** | **Rate**  **(Rs)** | **Amount**  **(Rs)** |
| 1 | 251 | Earth work in excavation in trenches for foundation of pipes | 76.25m3 |  |  |
| 2 | 303 | Class-150 brick work in 1:6 cement and fine sand of 1.25 finess modulus mortar in foundation and plinth including supply of all materials labour T&P etc. complete work | 60m3 |  |  |
| 3 | Item no-7 | Supply fine sand | 25 Cum |  |  |
| 4 | 17.58 | 12mm plaster in single coat in proportion of 1 cement : 6 fine sand | 160m2 |  |  |
| 5 | MR | S/F P.V.C pipe 4" heavy quality ISI mark supreme or equivalent make 6 Kg/m2 including all material, labour T&P etc required for proper completion of work | 305mtr |  |  |
| 6 | MR | Supply P.V.C Bend 4" heavy quality supreme or equivalent make | 03Nos |  |  |
| 7 | MR | Supply C.I Tee 4"×4"×4" ISI mark | 03Nos |  |  |
| 8 | MR | Supply G.I Reducer 4"×3" “B” class | 03Nos |  |  |
| 9 | MR | Supply C.I Sluice valve 4" heavy quality ISI mark | 04Nos |  |  |
| 10 | MR | Supply P.V.C socket 4" heavy quality ISI mark | 60Nos |  |  |
| 11 |  | Unseen work | LS |  |  |
| 12 |  | Labour charges for joining 04 C.I Sluice valves, C.I Tee etc including labour T&P complete work | 01 job |  |  |
|  |  |  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Connection of 10 HP submersible pump 2 Nos to OHT in both campus**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**