**H.B.T.I Kanpur**

**Tender Form**

Name of work- **Renovation of labs in Chemistry Deptt.**

Estimated cost- Rs 957127.00 Time of completion- 03 months Earnest money- Rs 20000.00

Tender form cost- Rs 1100.00

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl.No.** | **Schedule Item** | **Description Of Work** | **Quantity** | **Rate (Rs)** | **Amount (Rs)** |
| 1 | 704 | Dismantling doors and windows leaves including stacking of materials as directed by Engineer incharge | 32m2 |  |  |
| 2 | 310 | Class 150 brick work in 1 cement : 4 coarse sand in super structure above plinth level | 16.50m3 |  |  |
| 3 | 706 | Dismantling of existing plaster including disposal of refuse material | 142.8m2 |  |  |
| 4 | 697 | Dismantling C.C. or brick or granolithic floor including stacking of dismantling materials as directed by Engineer incharge | 153m2 |  |  |
| 5 | 17.59(iii) | 15 mm thick plaster on wall 1 : 6 cement and coarse sand | 150 m2 |  |  |
| 6 | 279 | P/L in CC 4 : 2 : 1 of not less than strength of M-150 (stone ballast 40 mm normal size) and curing complete work | 8.50m3 |  |  |
| 7 | Item No-24 | Reinforcement for cement and structural steel | 650Kg |  |  |
| 8 | 14.43(b)(23) | P/L of 8 to 10mm thick ivory or light shade vitrified tiles of 600×600mm size in flooring or skirting laid with 1 : 3 cement mortar(1cement : 3coarse sand) finishing with pigment cement slurry and with pigment grouting and polishing complete etc supply of all materials labour T&P required for proper completion of work | 130m2 |  |  |
| 9 | 14.43(b)(22) | 20mm thick marble tiles in risers of steps & skirting dodo wall and pillar laid on 10mm thick cement mortar 1:3 (1cement : 3 coarse sand) jointed with grey cement slurry mixed with pigment to match the shade of slabs including rubbing and polishing complete | 84m2 |  |  |
| 10 | Item no-14 | S/F white glazed fine clay sink 600×450×250mm | 6Nos |  |  |
| 11 | 502 | Fabrication and fixing of MS grill with MS angle 25×5×5mm framing with MS bar 8mm fixing at normal height | 450Kg |  |  |
| 12 | MR | Aluminum partition with 5mm thick glass for chamber and wardrobe under platform | 40.6m2 |  |  |
| 13 | MR | Aluminum fitting for partition work (sliding, bracket, hinges, hydraulics door closer etc) | LS |  |  |
| 14 | 708 | Scraping old white or colour washes including disposal of refuse materials | 260m2 |  |  |
| 15 | Item no-36 | P/L JK wall putty | 120Kg |  |  |
| 16 | 672 | White washing two coat | 180m2 |  |  |
| 17 | 649 | One Priming coat and one coat of oil distemper including supply of all materials labour T&P etc complete work | 520m2 |  |  |
| 18 | 651 | As in Sr.no-17 above but every coat after the first coat | 520m2 |  |  |
| 19 | Item no-2 | Providing and injecting chemical for past constructional anti termite treatment with drilling holes at junction of floor with walls and pillars | 108m2 |  |  |
| 20 | 641 | Painting two coat of ready mix paint on new iron work after one coat of ready mix primer | 30m2 |  |  |
| 21 | 812(b) | Fixing panes of glass with equal or equivalent ISI mark quality with putty brads and springs and including supply of material and labour etc complete work 3.8 to 4.7 mm thick | 35m2 |  |  |
| 22 |  | Unseen work and contingency | LS |  |  |
| 23 |  | Electrification work 5% |  |  |  |
| 24 |  | Plumbing work 5% |  |  |  |
|  |  |  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director

Name of work- **Renovation of labs in chemistry deptt.**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name ,Address and Mobile No. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**