**H.B.T.I Kanpur**

**Tender form**

Name of work- **Water proofing over the roof of Mechanical Engg. Deptt.**

 Estimated cost- Rs 1251600.00

Time of completion- 03 months Earnest money- Rs 25500.00

 Tender form cost- Rs 1500.00

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S.No.** | **Sch.No.** | **Description of work** | **Qty** | **Unit** | **Rate(Rs)** | **Amount(Rs)** |
| 1 | M.R. | Water proofing treatment over the roof **Specification-**1. Clean the previous surface properly with wire brush.
2. Providing and doing a coat of approved cold bitumen primer (make IWL of Pidilite or eqv.) @ 0.3 Ltr. per Sqm. over the entire dried area.
3. Providing and fixing App Polyester Membrane 2 mm thick (make- IWL or Pidilite or stp. or eqv.) on primed surface by **TORCH** application method and over lap must be 100 mm on the joint.
4. Providing and doing a coat of approved cold bitumen Primer (make- IWL or Pidilite 0r stp. or eqv.) @ 0.3 Ltr. per Sqm. over the polyester membrane and the fix the FIBER NET over on entire coated area with sand spreading to make the rough surface .
5. Providing and doing 25 mm thick cement sand plaster in ratio 1:3 (1 cement : 3 coarse sand) over the FIBER NET with Dr. Fixit Pidiproof LW-200 ML/cement Bag and floating coat of neat cement (Doga) with Dr. fixit Pidicreat MPB in ratio 10:1.
6. Making fo Gola all round roof far carrying the water proofing treatment upto groove.
7. Cutting and filling of groove over gola.
 | 1600 | Sqm |  |  |
| 2 |  | Contingency 5% | - | - |  |  |
|  |  |  |  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Water proofing over the roof of Mechanical Engg. Deptt.**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**