**H.B.T.I Kanpur**

**Tender Form**

Name of work- **Renovation of humanity HOD office**

 Estimated cost- Rs 194939.00

Time of completion- 01 months Earnest money- Rs 2500.00

 Tender form cost- Rs 550.00

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sch. PWD** | **Description of work** | **Qty** | **Rate(Rs)** | **Amt(Rs)** |
| 708 | **(a)** Scrapping old white or colour wash including disposal of refuse material as directed by Engineer in-charge with a distance 60m | 196M2 |  |  |
| 706 | **(b)** Dismantling existing plaster including disposal of refused material as directed by Engineer  | 39M2 |  |  |
| Chapter1 | Providing & laying two layer putty (Birla White or J.K) wall putty on surface including supply of all material as well as using emery paper as per requirement | 178M2 |  |  |
| 651 | Oil bond distemper two coat as previously old distemper surface including supply of all materials, labour and T&P etc required for proper completion of work | 196M2 |  |  |
| 17.63 | Plastering on ceilings (1 cement : 3 sand)  | 25M2 |  |  |
| 17.59 | 15 MM cement plaster in single coat on rough side of half brick wall | 22.95M2 |  |  |
| 643 | Previously paint old wood or steel work of approved super quality ready mixed paint of clear synthetic varnish including supply of all materials labour & T&P etc required for proper completion of work | 35M2 |  |  |
| Chapter-14/23 | P/L of 8 to 10mm thick ivory or light shade vitrified tiles of 600mm×600mm size in flooring of skirting laid with 1 : 3 cement mortar finishing with cement slurry with pigment grouding | 30M2 |  |  |
| 502 | Fabrication & fixing of MS grill with MS angle and MS bar(LS 58Kg) | 01Nos |  |  |
| 698 | Dismantling cement concrete or bricks or granolithic floors including concrete that floor to be stone flagged or tiled floors | 28M2 |  |  |
| MR | S/F of Aluminum partition with 5mm thick glass for chambers | 9M2 |  |  |
| MR | S/F Hydraulics door closer on aluminum partition 1Nos  |  01Nos |  |  |
| MR | Door lock with handle |  01Nos |  |  |
| MR | Blind curtain for window |  04Sqm |  |  |
| MR | Dismantling and further fitting after the completion of work on the another place as per requirement as well as repairing & gas filling  | LS |  |  |
| Chapter-21,22,23 | S/F of complete hand wash basin (550×400)mm | 01set |  |  |
| MR | Fixing of above MS item | 03job |  |  |
| Chapter-22 | Looking mirror(600×450)mm dia size make Atul |  01Nos |  |  |
| Chapter-21 | S/F of ‘B’ class G.I pipes and its related fittings  | LS |  |  |
|  | Electric work  | LS |  |  |
|  | Unseen work | LS |  |  |
|  | **Total**  |  |  |  |

**Terms & Conditions-**

1. All the work is to be executed as per PWD specification and norms.
2. The contractor should attached a copy of TIN No.
3. The contractor should attached a copy of PAN No. and copy of last year ITR.
4. The contractor should attached a copy of registration certificate of state/central govt.
5. An affidavit to the effect that firm is not black listed by any state/central Govt. Deptt.
6. Satisfactory working certificate is necessary for similar type of work and amount.
7. Annual turnover of the firm should be Rs 1.00 crore or more.
8. The quantity may increase or decrease as per decision of competent authority.
9. Without attachment of the above the tenders are not considered.
10. In case of unjustified quoted rate below the tender cost, tender will be considered non-responsive and his/her earnest money will be forfeited.
11. After allotment of said work security money (10%) will be deposited within a week, otherwise earnest money will be forfeited and work will allotted to second lowest.
12. Any query about tender can be made from institute during working day and time.
13. Payment will be made after completion and satisfactory report of the said work, running payment would made after satisfaction of work and recommendation of committee constituted by Director.

Name of work- **Renovation of humanity HOD office**

**Signature of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Name, Address & Mobile no. of Contractor\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**